Tender Specification: SLC-Motion203-C

Description:
Street light controller with integrated PIR motion sensor for connection to a Zhaga Book 18 interface, enabling demand-based control, monitoring and configuration of individual lighting assets.

Manufacturer: 	esave AG
Type: 	SLC-Motion203-C
	or approved equivalent
Certification: 	CE, Zhaga D4i, DALI-2

Function:
Street light controller with integrated PIR motion sensor for integrating individual LED luminaires into a wireless lighting management system. Enables light-on-demand functionality as well as monitoring, control, configuration and data collection through a self-organizing 2.4 GHz mesh network. The integrated GNSS receiver provides automatic positioning and time synchronization for location-based lighting functions. An integrated eSIM enables remote connectivity, monitoring and gateway operation for up to 100 connected luminaires..

Configuration can be performed locally using a commissioning software or remotely via web platform.

Installation:
-	Installation via Zhaga interface (Book 18)
-	Tool-free plug-and-play installation

Technical Data:
-	Supply voltage: 	12 – 30 V DC | typ. 24 V DC
-	Current consumption: 	16 – 45 mA
-	Power consumption: 	typ. 450 mW
-	Operating temperature: 	–40 … +80 °C
-	Protection class: 	IP66
-	Impact resistance: 	IK09

Wireless Communication (2.4 GHz Mesh):
-	Frequency range: 	2.420 – 2.480 GHz
-	Standard: 		IEEE 802.15.4
-	RF output power: 	+8 dBm
-	Receiver sensitivity: 	–100 dBm

Cellular Communication:
-	Protocols: LTE Cat M1, NB-IoT NB2, EGPRS
-	Integrated eSIM supporting worldwide cellular connectivity

Housing:
-	Material: 		Polycarbonate / PBT
-	Color: 		Transparent smoke grey
-	Diameter: 		81.5 mm
-	Height: 		44 mm
-	Weight: 		80 g

Features:
Configuration
-	Local commissioning, configuration and firmware updates 
-	Over-the-air firmware updates for controllers managed through the SL-Control web platform
-	Remote access and status monitoring via cellular connectivity and the SL-Control web platform
-	Automatic positioning and time synchronization via GNSS
Connectivity
-	Gateway functionality for up to 100 connected luminaires
-	Networked lighting control via a self-organizing 2.4 GHz mesh network
-	AES-128 encrypted wireless communication 
Sensors
-	Integrated brightness sensor 
-	Integrated tilt sensor 
-	Integrated temperature sensor 
-	Integrated PIR Motion Sensor
DALI 
-	DALI-2 and D4i certified application controller, compliant with DALI Part 351 Type A
-	Supports DALI Part 303 occupancy sensors and DALI Part 304 light sensors
-	Supports DALI DT6, DT7, and DT8 control gear
Lighting
-	AstroDim function with automatic calculation of local sunrise and sunset times
-	Responds to motion and sensor events across the mesh network
-	Distribution of brightness and sensor data across the mesh network