Tender Specification: Zhaga Dual Connection Box

Description:
External connection box with two standardized Zhaga Book 18 interfaces for the installation of compatible controllers on poles or walls.

Manufacturer: 	esave AG
Type: 	Zhaga Dual Connection Box
	or approved equivalent
Certification: 	CE

Function:
The Connection box provides two Zhaga Book 18 interface located on the bottom of the housing for the external installation of compatible controllers. It enables existing luminaires to be equipped with a standardized external interface, allowing compatible devices to be connected easily via plug-and-play connection.

The robust, weather-resistant housing is designed for outdoor applications and enables flexible mounting on poles or walls.

Mounting:
-	Pole or wall mounting

Technical Data:
-	Supply Voltage: 	100 – 277 V AC
-	Max. Supply Voltage: 	305 V AC
-	Max. Input Current: 	150 mA
-	DALI Input Current: 	max. 240 mA
-	Storage Temperature:	 –20 … +85 °C
-	Fire Class: 	UL 94 HB V-2
-	Surge Protection:	6 kV, 2 Ω (10 pulses according to IEC 62368-1)

Housing:
-	Material: 		Polycarbonate (PC)
-	Color: 		Black
-	Length: 		104 mm
-	Width:		88 mm
-	Height: 		152 mm
-	Membrane:	PTFE
-	Cable Gland:	Polyamide

Interfaces:
-	Two Zhaga Book 18 interfaces

DALI:
-	Integrated DALI power supply for the DALI bus