Tender Specification: Zhaga Top Connection Box

Description:
External connection box featuring one top-mounted standardized Zhaga Book 18 receptacle for the installation of compatible controllers on poles or walls.

Manufacturer: 	esave AG
Type: 	Zhaga Top Connection Box
	or approved equivalent
Certification: 	CE

Function:
The Zhaga Top Connection box provides an external Zhaga Book 18 receptacle located on the top of the housing for the installation of compatible controllers. It enables existing luminaires to be equipped with standardized external receptacles, allowing compatible controllers and sensors to be installed quickly and easily through plug-and-play connections without modification to the luminaire housing.

The robust, weather-resistant housing is designed for reliable outdoor applications and supports flexible installation on poles or walls.

Mounting:
-	Pole or wall mounting

Technical Data:
-	Supply Voltage: 	100 – 277 V AC
-	Max. Supply Voltage: 	305 V AC
-	Max. Input Current: 	150 mA
-	DALI Input Current: 	max. 240 mA
-	Storage Temperature:	 –20 … +85 °C
-	Fire Class: 	UL 94 HB V-2
-	Surge Protection:	6 kV, 2 Ω (10 pulses according to IEC 62368-1)

Housing:
-	Material: 		Polycarbonate (PC)
-	Color: 		Black
-	Length: 		104 mm
-	Width:		92 mm
-	Height: 		152 mm
-	Membrane:	PTFE
-	Cable Gland:	Polyamide

Receptacles:
-	One Zhaga Book 18 receptacle, located on the top of the housing

DALI:
-	Integrated DALI power supply for the DALI bus