Tender Specification: NEMA Connection Box

Description:
External connection box featuring one NEMA receptacle for the installation of compatible controllers on poles or walls.

Manufacturer: 	esave AG
Type: 	NEMA Connection Box
	or approved equivalent
Certification: 	CE

Function:
The NEMA Connection box provides an external NEMA receptacle for the installation of compatible smart lighting controllers. It enables existing luminaires to be equipped with a standardized external connection point, allowing controllers to be installed quickly and easily via plug-and-play connection.

The robust, weather-resistant housing is designed for reliable outdoor operation and supports flexible installation on poles or walls.

Mounting:
-	Pole or wall mounting

Technical Data:
-	Supply Voltage: 	100 – 277 V AC
-	Max. Supply Voltage: 	305 V AC
-	Max. Input Current: 	150 mA
-	DALI Input Current: 	max. 240 mA
-	Storage Temperature:	 –20 … +85 °C
-	Fire Class: 	UL 94 HB V-2
-	Surge Protection:	6 kV, 2 Ω (10 pulses according to IEC 62368-1)

Housing:
-	Material: 		Polycarbonate (PC)
-	Color: 		Black
-	Length: 		104 mm
-	Width:		92 mm
-	Height: 		163 mm
-	Membrane:	PTFE
-	Cable Gland:	Polyamide

Receptacles:
-	One NEMA receptacle

DALI:
-	Integrated DALI power supply for the DALI bus